REVISION 6 & 7 NOTES

Highlights of Change:

Cover – Updated Revision Status to Rev 7
Page iv – Updated RECORD OF REVISIONS
Pages vi thru xi - Updated LOG OF EFFECTIVE PAGES to reflect Rev 7 – Changes indicated by dates
Preamble Pages 4-1 thru 4-6.  Removed 50-hour references and change verbiage on NOTE’s
A0051.4 Page 2 – Removed ASB Reference for Pillow Block Torque check – Incorporated into MM Chp 4.
A0052 Page 3 – Moved A0052.7 HYDRAULIC to A0054 to even out inspections
A0052 Page 4 – Cleaned up verbiage in A0052.8 differentiating types of driveshafts
A0052 Page 5 – Moved A0052.11 Lubrication to A0100
A0053 Page 2 - Removed Pillow Block Torque Check – Now incorporated into MM Chp 4
A0053 Page 2 - Moved A0053.6 DRIVETRAIN to A0054.5 renamed TAIL ROTOR DRIVETRAIN. Moved Oil cooler blower impeller, shaft and bearings to A1720
A0053 Page 3 -– Moved A0054.5 TAILBOOM STRUCTURE to A0053.8
A0053 Page 3 – Moved A0053.6.2 & 6.3 to A1720
A0053 Page 4  – Merged A0054.7 TAIL ROTOR GEARBOX and A0054.8 TAIL ROTOR PITCH CHANGE CONTROL into A0053.9 TAIL ROTOR GEARBOX
A0054 Page 1 – Changed A054.5 TAIL ROTOR DRIVETRAIN to FREEWHEELING UNIT 
A0054 Page 2 – Removed 100 hour tailboom inspection Tracked as AD2013-25-10 in Status Sheets 
A0054 Page 2 – Added HYDRAULIC from A0052
A0054 – All pages effected globally, now only 4 pages – All Rev 7
A0054 Page 3 – Moved A0055.8.1 Pillow blocks to A0100 (Chp 4 - 110 hour requirement)
A0056 Page 3 – Removed A0056.7 LUBRICATION. Now C/W every 100 hours in A0100
A0100 added to track 100 hour items (bulk is lubes).
A1720 Page 2 – Added Oil Cooler impeller, shaft and bearings.  Repaginated A1720
A1720 Page 2 – Added step 4.9.9.2
A6010 Removed – Now tracked on Status Sheets. Part comes off, overhauled then put into rotables.
B0051NT Page 2 – Added inspection to starter generator duct and clamp.
B0051.5NT Page 4 – Removed Compressor Fresh Water Rinse
[bookmark: _GoBack]B0052.6NT Page 4 – Removed Compressor Fresh Water Rinse
B0053.4NT Page 4 – Removed Compressor Fresh Water Rinse
B0054.4NT Page 4 – Removed Compressor Fresh Water Rinse
B0055.5NT Page 4 – Removed Compressor Fresh Water Rinse
B0056.4NT Page 4 – Removed Compressor Fresh Water Rinse
NOTE: Engine washes will now be tracked on MHI CALM aircraft status report at 100 hour intervals.
B0056NT Page 2 – Removed B0056.3.1.11 already covered in B0055.4.14  (duplicate)
C0100 Added for 100 hour NVG inspection.
C1700 – 12 Mon Insp - All pages renamed to reflect correct AAIP 12-month designator, now C 1700
C1710 – Added for 12 Mon NVG inspection.
C1720 Page 7 – Added C1720.18 AAI TAIL ROTOR LOCKOUT KIT (currently tracked on status report)
C1720 Page 8 – Added C1720.19 AAI LOCKING FUEL CAP (currently tracked on status report)
Attachment A-1 – Added #1 ASU Night Vision Goggle Lighting System, #6 AAI TAIL ROTOR LOCKOUT KIT, #7 AAI LOCKING FUEL CAP and #24 DART AVIONICS CONSOLE (all currently tracked on status report)
Attachment B – Added Rolls-Royce Engine Wash to INSPECTIONS EXCLUDED FROM AAIP.  Engine washes will now be tracked on MHI CALM aircraft status report at 100 hour intervals.

