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	1.
	Headset/

Helmet Hooks
D
	2
	0
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	2.
	EPIRB Bracket
D
	1
	0
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	3.
	EPIRB

D
	1
	0
	May be deferred.
	NONE
	NONE
	NONE
	Overwater flight prohibited.

	4.
	Approach Plate Holder
D
	2
	0
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	5.
	Approach Plate Light
D
	2
	0
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	6..
	Checklist Holder
D
	1
	0
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	7.
	Crew Door Pull Handle

D
	2
	0
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	8.
	Alerts
D
	1
	0
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	9.
	Seat covers and/or cushions

D
	--
	0
	May be deferred.
	NONE
	NONE
	NONE
	Neither the seat framework, nor crash attenuation properties may be compromised.

	10.
	Loose or missing weather stripping or door seals

D
	--
	0
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	11.
	Snap Vents

D
	--
	0
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	12.
	Throttle grip covering

D
	--
	0
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	13.
	Control Switch Knob
D
	--
	--
	May be deferred.
	NONE
	NONE
	NONE
	Limitations: May not be missing.  If broken it must remain securely attached and functional.  No part of the knob may be missing which provides a visual indication of its position.

	14.
	Buttons, Knobs, Switches

D
	--
	--
	Which are part of a larger assembly, but do not control anything may be deferred.
	NONE
	NONE
	NONE
	NONE

	15.
	Interior Trim Panels

D
	--
	--
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	16.
	Door Struts

D
	--
	--
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	17. 
	Heating, Ventilation, and defogging gaspers and vents.

D
	--
	--
	May be deferred.
	NONE
	NONE
	NONE
	Airflow must be controlled at some other point.
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	18.
	Heater/
Defroster knobs
D
	--
	--
	May be deferred.
	NONE
	NONE
	NONE
	Heater/Defroster use will not be needed for intended flight.

	19.
	Map Light

D
	--
	--
	May be deferred
	NONE
	NONE
	NONE
	NONE

	20.
	Cargo Hook Load Indicator (Load Cell)

D
	--
	--
	May be deferred
	NONE
	NONE
	NONE
	NONE

	21.
	Window Tension Knob(s)

D
	--
	--
	May be deferred
	NONE
	NONE
	NONE
	NONE

	22.
	Standby Compass Light

D
	--
	--
	May be deferred
	NONE
	NONE
	NONE
	NONE
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	23.
	Cyclic Boot

D
	--
	--
	May be deferred
	NONE
	NONE
	NONE
	NONE

	24.
	Dual Control Collective Cover

D
	--
	--
	May be deferred
	NONE
	NONE
	NONE
	NONE

	25.
	Door Mirrors

D
	--
	--
	May be deferred
	NONE
	NONE
	NONE
	NONE

	26.
	Magnetic Compass

Housing

D
	--
	--
	May be deferred
	NONE
	None
	NONE
	NONE

	27.
	HTAWS

D
	--
	--
	May be inoperative
	NONE
	Install Orange dot on HTAWS control head
	NONE
	NONE
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	28.
	Seatbelt Tags

D
	--
	--
	May be worn/faded
	NONE
	NONE
	NONE
	NONE

	29.
	Other Items

D
	--
	--
	Refer to Flowchart.
	NONE
	NONE
	NONE
	Complete Flowchart and if its determined that the item is an NEF item,  Defer the item IAW the NEF program.
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