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1.          NEF PROGRAM

Instruction below outline the Maritime Helicopters NEF program. 

2.	SYSTEM DEFINITIONS

a.	By definition, NEF items do not affect the safe operation of an aircraft.  Due to the wide variance of these items from aircraft to aircraft, a complete list of NEF items is not required to be maintained in the operator’s MEL, but in a list or other equivalent method of tracking.

b. A vertical bar (change bar) in the margin indicates a change, addition or deletion in the adjacent text for the current revision of that page only.  The change bar is dropped at the next revision of that page.

3.	REPAIR INTERVALS

CATEGORY A:  Items in this category shall be repaired within the time interval specified in the remarks column of the operator's approved MEL.   For time intervals specified in “flight days” the day the malfunction was recorded in the aircraft maintenance record/logbook is excluded.  For all other time intervals (flights, flight legs, cycles, hours, etc), repair tracking begins at the point when the malfunction is deferred in accordance with the operator’s approved MEL. 

CATEGORY B:  Items in this category shall be repaired within three (3) consecutive calendar days (72 hours), excluding the day the malfunction was recorded in the aircraft maintenance record/logbook.  For example, if it were recorded at 10 AM on January 26th, the three day interval would begin at midnight the 26th and end at midnight the 29th.

CATEGORY C:  Items in this category shall be repaired within ten (10) consecutive calendar days (240 hours), excluding the day the malfunction was recorded in the aircraft maintenance record/logbook.  For example, if it were recorded at 10 AM on January 26th, the 10 day interval would begin at midnight the 26th and end at midnight February 5th.

CATEGORY D:  Items in this category shall be repaired within one hundred twenty (120) consecutive calendar days (2880 hours), excluding the day the malfunction was recorded in the aircraft maintenance record/logbook.  The letter designators are inserted adjacent to Column 2.

4. OTHER ITEMS.  

Items that are found routinely identified as “Not on the List” will be evaluated utilizing the following flow chart. The qualified items will then be added to the NEF deferral list during the next revision of this document.
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	1.
SEQUENCE
NUMBERS
	2.
ITEM
	3.
     QUANTITY
INST         REQD
	4.
REMARKS  AND
EXCEPTIONS
	5.
DEACTIVATION
PROCEDURE
	6.
PLACARDING
	7.
PROCEDURE
	8.
OPS LIMITS

	1.
	Headset/
Helmet Hooks
D
	2
	0
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	2.
	Approach Plate Holder
D
	2
	0
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	3.
	Approach Plate Light
D
	2
	0
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	4..
	Checklist Holder
D
	1
	0
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	5.
	Crew Door Pull Handle
D
	2
	0
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	6.
	Seat covers and/or cushions
D
	--
	0
	May be deferred.
	NONE
	NONE
	NONE
	Neither the seat framework, nor crash attenuation properties may be compromised.

	7.
	Loose or missing weather stripping or door seals
D
	--
	0
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	8.
	Snap Vents
D
	--
	0
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	9.
	Throttle grip covering
D
	--
	0
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	10.
	Control Switch Knob
D
	--
	--
	May be deferred.
	NONE
	NONE
	NONE
	Limitations: May not be missing.  If broken it must remain securely attached and functional.  No part of the knob may be missing which provides a visual indication of its position.

	11.
	Buttons, Knobs, Switches
D
	--
	--
	Which are part of a larger assembly, but does not control primary function.
	NONE
	NONE
	NONE
	NONE

	12.
	Interior Trim Panels
D
	--
	--
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	13.
	Door Struts
D
	--
	--
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	14. 
	Heating, Ventilation, and defogging gaspers and vents.
D
	--
	--
	May be deferred.
	NONE
	NONE
	NONE
	Airflow must be controlled at some other point.

	15.
	Heater/
Defroster knobs
D
	--
	--
	May be deferred.
	NONE
	NONE
	NONE
	Heater/Defroster use will not be needed for intended flight.

	16.
	Map Light
D
	--
	--
	May be deferred
	NONE
	NONE
	NONE
	NONE

	17.
	Cargo Hook Load Indicator (Load Cell)
D
	--
	--
	May be deferred
	NONE
	NONE
	NONE
	NONE

	18.
	Window Tension Knob(s)
D
	--
	--
	May be deferred
	NONE
	NONE
	NONE
	NONE

	19.
	Standby Compass Light
D
	--
	--
	May be deferred
	NONE
	NONE
	NONE
	NONE

	1.
SEQUENCE
NUMBERS
	2.
ITEM
	3.
      QUANTITY
INST            REQD
	4.
REMARKS  AND
EXCEPTIONS
	5.
DEACTIVATION
PROCEDURE
	6.
PLACARDING
	7.
PROCEDURE
	8.
OPS LIMITS

	20.
	Cyclic Boot
D
	--
	--
	May be deferred
	NONE
	NONE
	NONE
	NONE

	21.
	Dual Control Collective Cover
D
	--
	--
	May be deferred
	NONE
	NONE
	NONE
	NONE

	22.
	Door Mirrors
D
	--
	--
	May be deferred
	NONE
	NONE
	NONE
	NONE

	23.
	Magnetic Compass
Housing
D
	--
	--
	May be deferred
	NONE
	None
	NONE
	NONE

	24.
	HTAWS
D
	--
	--
	May be inoperative
	NONE
	Install Orange dot on HTAWS control head
	NONE
	NONE

	25.
	Seatbelt Tags
D
	--
	--
	May be worn/faded
	NONE
	NONE
	NONE
	NONE

	26.
	Other Items
D
	--
	--
	Refer to Flowchart.
	NONE
	NONE
	NONE
	Complete Flowchart and if its determined that the item is an NEF item,  Defer the item IAW the NEF program.
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	1
SEQUENCE NUMBERS
	2
          ITEM
	3
      QUANTITY
INST            REQD
	4
REMARKS  AND
EXCEPTIONS
	5
DEACTIVATION
PROCEDURE
	6
PLACARDING
	7
PROCEDURE
	8
OPS LIMITS

	1.
	Headset/
Helmet Hooks
D
	--
	--
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	2.
	Passenger Headset Jacks
D
	--
	--
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	3.
	Cabin Lighting/
Signs (Reading lights, Light Lens/Covers)
D
	--
	0
	Only items not covered by MEL ATA 33.
	NONE
	NONE
	NONE
	NONE



	4.
	Door Latch Guard Covers
D
	--
	0
	May be deferred, provided they are not an integral part of the actual door latch and do not interfere wit operation of the door latch.
	NONE
	NONE
	NONE
	NONE

	5.
	Floor Liners
D
	--
	0
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	6.
	Seat covers and/or cushions
D
	--
	0
	May be deferred.
	NONE
	NONE
	NONE
	Neither the seat framework, nor crash attenuation properties may be compromised.

	7..
	Loose or missing weather stripping or door seals
D
	--
	0
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	8.
	Snap Vents
D
	--
	0
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	9.
	Interior Trim Panels
D
	--
	--
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	10.
	Door Struts
D
	--
	--
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	11. 
	Heating, Ventilation, and defogging gaspers and vents.
D
	--
	--
	May be deferred.
	NONE
	NONE
	NONE
	Airflow must be controlled at some other point.






	1
SEQUENCE NUMBERS
	2
ITEM
	3
     QUANTITY
  INST            REQD
	4
REMARKS  AND
EXCEPTIONS
	5
DEACTIVATION
PROCEDURE
	6
PLACARDING
	7
PROCEDURE
	8
OPS LIMITS

	12.
	Cabin Door Slider(s)
D
	--
	--
	Door must still function properly.
	NONE
	NONE
	NONE
	NONE

	13.
	Other Items
D
	--
	--
	Refer to Flowchart.
	NONE
	NONE
	NONE
	Complete Flowchart and if its determined that the item is an NEF item,  Defer the item IAW the NEF program.
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	1
SEQUENCE NUMBERS
	2
ITEM
	3
      QUANTITY
INST             REQD
	4
REMARKS  AND
EXCEPTIONS
	5
DEACTIVATION
PROCEDURE
	6
PLACARDING
	7
PROCEDURE
	8
OPS LIMITS

	1.
	Floor Liners
D
	--
	0
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	2.
	Tie Down Bags
D
	--
	0
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	3.
	Loose or Missing Weather Stripping or Door Seals
D
	--
	0
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	4.
	Interior Trim Panels
D
	--
	--
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	5.
	Door Retention Straps
D
	--
	--
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	7.



.
	Interior Baggage Canvas/Net Covers/
Restraints
D
	--
	--
	May be deferred.
	NONE
	NONE
	NONE
	Cargo must be restrained by alternate means.

	8.
	Sidewall panel or extender
D
	--
	--
	May be deferred
	NONE
	NONE
	NONE
	NONE

	9.
	Baggage Compartment damage
D
	--
	--
	Damage classification must be negligible or repairable.
	Damage must be protected from further damage by protecting the area with sealant tape
	NONE
	NONE
	NONE

	10.
	Baggage Compartment
Door damage
D
	--
	--
	Damage classification must be negligible or repairable.  
Damage cannot exceed the number of repairs listed in applicable manufactures manuals
	Damage must be protected from further damage by protecting the area with sealant or tape.
	NONE
	NONE
	NONE

	11.
	Other Items
D
	--
	--
	Refer to Flowchart.
	NONE
	NONE
	NONE
	Complete Flowchart and if its determined that the item is an NEF item,  Defer the item IAW the NEF program.
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BAGGAGE CARGO COMPARTMENT



	1
SEQUENCE NUMBERS
	2
ITEM
	3
        QUANTITY
  INST            REQD
	4
REMARKS  AND
EXCEPTIONS
	5
DEACTIVATION
PROCEDURE
	6
PLACARDING
	7
PROCEDURE
	8
OPS LIMITS

	1.
	Faded or missing paint
D
	--
	0
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	2.
	External Cargo Mirror(s)
D
	--
	0
	May be deferred, integrity of installation must not be effected or mirror removed.
	NONE
	NONE
	NONE
	External Load operations will not be conducted.

	3.
	Rear view mirror(s)
D
	--
	0
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	4.
	Cargo Hook
D
	--
	0
	May be deferred.
	NONE
	NONE
	NONE
	External Load operations will not be conducted.

	5.
	Lights
D
	--
	--
	Only items not covered by MEL ATA 33.
	NONE
	NONE
	NONE
	NONE

	6.
	Tail Rotor Gear Box Dust Boot
D
	--
	0
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	7.
	Cowl Door Latch
C
	--
	0
	May be deferred.
	NONE
	NONE
	NONE
	Only one latch per cowling may be deferred.

	8.
	Hydraulic Servo Boot Torn
D
	--
	0
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	9.
	Starter/ Generator Exhaust Duct Seal
D
	--
	0
	May be deferred
	NONE
	NONE
	NONE
	NONE

	10.
	Static Port Heaters (Bell 407 Only)
C
	2
	0
	May be inoperative provided: 
1.  Pitot heat is not required to be on IAW the RFM.
	Turn Pilot Heat Off.
	Install orange dot on pitot heater switch
	NONE
	No flights in visible moisture when temperature is below +4 degrees Celsius.  

	11.
	Tanis Heater 
D
	1
	0
	May be deferred.
	NONE
	NONE
	NONE
	NONE

	12. 
	Starter/  Generator drain line
D
	1
	--
	May be damaged 
	NONE
	NONE
	NONE
	NONE













	1
SEQUENCE NUMBERS
	2
ITEM
	3
      QUANTITY
INST           REQD
	4
REMARKS  AND
   EXCEPTIONS
	5
DEACTIVATION
     PROCEDURE
	6
PLACARDING
	7
PROCEDURE
	8
OPS LIMITS

	13.
	Main Rotor Blade Bolt Cap
D
	--
	--
	May be damaged
	NONE
	NONE
	NONE
	NONE



	14.
	Electrical Fuel Sump Drain Rubber Cover
D
	--
	--
	May be damaged or missing
	NONE
	NONE
	NONE
	NONE

	15.
	Other Items
D
	--
	--
	Refer to Flowchart.
	NONE
	NONE
	NONE
	Complete Flowchart and if its determined that the item is an NEF item,  Defer the item IAW the NEF program.
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