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ADDING AN AIRCRAFT TO AIR CARRIER OPERATIONS
Dear Applicant:
To add an aircraft to an air carrier operation the certificate holder must complete the following four steps.  
1 Decide the kinds of operations you intend with the aircraft and prepare a written statement showing that the aircraft and its equipment conforms to the requirements of FAR 135.25(a), including registration, current airworthiness certification, identification, and current airworthy condition.  The certificate holder must also show that it meets the requirements for all intended operations.  
2 Use OST Forms 4507 and 6410 to initiate or update your Air Carrier Registration with FAA Headquarters, Air Transportation Division AFS-260, 800 Independence Avenue SW, Washington, DC 20591.  Register and identify each aircraft used and keep the registration current.  
For blank forms go to. http://www.faa.gov/about/office_org/headquarters_offices/avs/offices/afs/afs200/branches/afs260/exemptions/
  
See FSIMS 8900.1 Volume 2 Chapter 2 Sections 1 and 2:  go to http://fsims.faa.gov/PICResults.aspx?mode=EBookContents.
3 Provide copies of the documents prepared in steps 1 and 2 to the FSDO and receive Operations Specifications Paragraph D85 and any other Operations Specifications that may be required (see below).  
4 Comply with FAR 135.63(a)(3) by adding the aircraft, including the kinds of operations authorized for the aircraft, to your official control-listing of aircraft used or available for use in air carrier operations. 
The attached documents, Notice of Intent to Add an Aircraft and Aircraft Compliance Statement for FAR 135 Operations, will help you accomplish steps 1 and 3.  They provide a means to document compliance and provide the information we need to issue all necessary Operations Specifications.  
THE INFORMATION REQUESTED IN THESE FORMS IS REQUIRED. You may use any method that provides complete and accurate information. However, the forms provided here give you an organized means to provide the FSDO the information it needs to issue the appropriate Operations Specifications. 
ACCURACY IS IMPORTANT: The Director of Maintenance should complete the document in consultation with the Director of Operations.  The Director of Maintenance should sign the statement on page 4-1 signifying complete and accurate technical information.  Consult with qualified specialists as needed for special operations or special means of navigation.  Technical errors or omissions can cause unnecessary delays to completion of the project.  
The SCHEDULE OF EVENTS on page 1-1 lists the events that may relate to adding the aircraft to your 135 operation.  If you schedule those events on this form, we will be able to determine our ability to meet your expectations and schedule our resources.  We will contact you if there are scheduling difficulties.  
We hope you find these forms useful in helping you determine aircraft eligibility and as a way to apply for certain kinds of operations.  Please let us know if you have any questions or suggestions.
	Sincerely, 


The Anchorage FSDO
	INSTRUCTIONS:  These forms are designed for manual or on-screen fill-in. For on-screen fill-in, use TAB and SHIFT-TAB and the mouse to navigate forward and back through the forms.  We suggest that you print a copy for reference while working on the document on your computer.  We also recommend saving the document with a new name before you start working on it to preserve the blank original.  Print the completed copy, sign, and send it to us.  
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	[bookmark: _Toc16496419]
OPERATOR AND AIRCRAFT INFORMATION
	Operator
Name
	     
	Certificate 
Number
	     

	
	Aircraft Make
	Complete Model Number
	Serial No
	Registration Number

	
	     
	     
	     
	N     

	
	Total Aircraft Time
	No 1.           Engine Time(s)         No. 2
	No 1.       Propeller Time(s)       No. 2

	
	      Hrs
	      Hrs
	      Hrs
	      Hrs
	      Hrs

	
	Registered Owner 
(see NOTE below)
	     

	
	Address
	     

	
	
	     

	
	City
	     
	State    
	ZIP      -    



NOTE:	If the aircraft owner's registered name is not exactly the same as the certificate holder’s legal name the applicant must show how she or he will control the operation and maintenance of the aircraft.  Show this by providing a copy of a lease or other agreement. 

	1.1 [bookmark: _Toc533324463][bookmark: _Toc533324644][bookmark: _Toc16496420]
DOCUMENTS REQUIRED AT SUBMISSION OF THIS NOTICE
See Section 2 for indications of the need for new or revised Procedures Manuals and Training Programs
		Document Included
	Not Applicable
	
		Document included
	Not Applicable
	

	
	[bookmark: Check63]|_|	Minimum Equipment List/revision	|_|
	[bookmark: Check67]|_|	Approved Aircraft Inspection Program 
(Turbine Powered Aircraft) 	|_|

	
	[bookmark: Check64]|_|	Maintenance Program/Revision	|_|
	[bookmark: Text33][bookmark: Check68]Other (list)      	|_|

	
	[bookmark: Check65]|_|	Copy of aircraft lease, letter of intent, or other agreement (see NOTE above)	|_|
	[bookmark: Check69]|_|	Continuous Airworthiness Maintenance Program 
(Required for Ten-or-More PAX optional for other operations)	|_|

	
	[bookmark: Check66]|_|	Operations Manual/Revisions	|_|
	[bookmark: Check70]|_|	Approved De-icing/Anti-icing Procedures/rev.	|_|



	[bookmark: _Toc533324464][bookmark: _Toc533324645][bookmark: _Ref2127017][bookmark: _Ref2127029][bookmark: _Toc16496421]
SCHEDULE OF EVENTS
If an event or item is applicable please enter your estimated date otherwise leave blank.
	PHASE 3  DOCUMENT COMPLIANCE 
	PHASE 4  DEMONSTRATION & INSPECTION
All documents must be approved or accepted before this phase

	
	EVENT
	PLANNED SUBMISSION DATE
	EVENT
	PLANNED SUBMISSION DATE

	
	Deviation Request  
(For Proving Test flights)
	     
	Pilot training 
	     

	
	Pilot Training Program/revision 
	     
	Maintenance training
	     

	
	Maintenance Training Program
	     
	FAA Conformity Inspection
	     

	
	Proving Test  or Validation Plan
	     
	Proving Test Flights
	     

	
	Final Compliance Statement 
	     
	Proficiency/Flight Checks
	     

	
	Insurance Registration with AFS-260, using OST Forms 4507 and 6410 (see cover letter)
NOTE: After initial certification, the date may may be up to 30 days after adding an additional aircraft 
	     
	Validation Test Flights  
	     

	
	
	
	[bookmark: Text36]     
	     

	
	
	
	     
	     

	
	PHASE 5 FAA CERTIFICATION and/or OPS SPECS
	PROPOSED COMPLETION DATE 
     



	[bookmark: _Toc16496422]
CONTACT 
INFORMATION
	NAME
	Phone & EMAIL ADDRESS

	
	Director of Maintenance
	     
	Phone:
	[bookmark: Text5](   )-     

	
	
	
	EMAIL:
	[bookmark: Text6]     

	
	
	
	FAX
	(   )-     

	
	Director of Operations
	     
	Phone:
	(   )-     

	
	
	
	EMAIL:
	     

	
	
	
	FAX
	(   )-     


Submitted by
[bookmark: Text31][bookmark: Text32]      (signature): __________________________________     Title:      	 Date:        	


[bookmark: _Toc533324462][bookmark: _Toc533324643]Page 1-1
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Formdate 
[bookmark: _Toc533324466][bookmark: _Toc533324647][bookmark: _Toc16496423]REQUEST FOR OPERATIONS SPECIFICATIONS 
FOR THIS AIRCRAFT

	[bookmark: _Toc533324467][bookmark: _Toc533324648][bookmark: _Toc16496424]
INTENDED KINDS 
OF OPERATIONS:
	


Cargo Only
(Never Passengers)
	Maximum Passenger
 Seating Capacity 
	

Day Only
	


Day/Night

	
	[bookmark: Check45][bookmark: Check46]
|_| YES  |_| NO
	[bookmark: Text2]   
	
|_| YES  |_| NO
	
|_| YES  |_| NO


[bookmark: _Hlt2128011]
	[bookmark: _Hlt2128037][bookmark: _Toc533324468][bookmark: _Toc533324649][bookmark: _Toc16496425][bookmark: _Hlt2128082][bookmark: _Hlt533324673]
AIRCRAFT OPERATIONS
	INSTRUCTIONS 
1.  If you want an operation described below, check the box to the left of its description.
	Document Requirements
	Procedures

	[bookmark: _Toc533324469][bookmark: _Toc533324650][bookmark: _Toc535287259][bookmark: _Toc2058550][bookmark: _Toc2058890][bookmark: _Toc2065074][bookmark: _Toc2125933][bookmark: _Toc2126332][bookmark: _Toc2126567][bookmark: _Toc2127156][bookmark: _Toc2128415][bookmark: _Toc2130675][bookmark: _Toc2131331][bookmark: _Toc2756191][bookmark: _Toc3695940][bookmark: _Toc6902480][bookmark: _Toc14228093][bookmark: _Toc14229321][bookmark: _Toc16496067][bookmark: _Toc16496426]
	
	
	
	Training/
Skill

	[bookmark: _Toc533324470][bookmark: _Toc533324651][bookmark: _Toc535287260][bookmark: _Toc2058551][bookmark: _Toc2058891][bookmark: _Toc2065075][bookmark: _Toc2125934][bookmark: _Toc2126333][bookmark: _Toc2126568][bookmark: _Toc2127157][bookmark: _Toc2128416][bookmark: _Toc2130676][bookmark: _Toc2131332][bookmark: _Toc2756192][bookmark: _Toc3695941][bookmark: _Toc6902481][bookmark: _Toc14228094][bookmark: _Toc14229322][bookmark: _Toc16496068][bookmark: _Toc16496247][bookmark: _Toc16496427]
	
	
	2.  Then, look to see if a   appears to the right of the operation under “Procedures” and/or “Training/Skill” and revise your operating procedures and training manual and prepare to show proficiency as indicated.   The FSDO will provide any guidance you request.  
	
	
	OPSS
Ref/
Par

	
	[bookmark: _Ref533230231][bookmark: _Toc533324471][bookmark: _Toc533324652]PART A  GENERAL

	
	CREW

	[bookmark: Check56]|_|	Conduct certain FAR 135 operations in accordance with flight and rest time limitations under 14 CFR Sections 135.261 through 135.273.
	
	
	A033

	
	
	|_|
	Make arrangements with training centers and other organizations for certificate holder training in accordance with 14 CFR Section 135.324.
If applicable, provide the FAR 142 Training Center information below or attach a list with the indicated information.  
	
	
	A031

	
	
	
	Name
	Certificate 
number
	Address
	Course name(s)
	
	
	

	
	
	
	     
	     
	     
     
	     
     
	
	
	

	
	
	|_|	Use an approved computer-based flight Crew recordkeeping system for FAR 135 operations
	
	
	A025

	
	
	|_|	Use an autopilot in lieu of a second-in-command.  Provide the following 
	Autopilot Make/Model 	       /      .	Date Installed       .
|_|	Please furnish a copy (cover page only) of the Flight Manual Supplement that identifies the aircraft and the autopilot.
|_|	Unless the autopilot is aircraft manufacturer installed, please furnish a copy of the FAA Form 337 showing the installation data.
	
	
	A015

	
	ICING

	|_|	Conduct a pretakeoff contamination check during ground icing conditions for Part 135 Operators.
	
	
	A041

	
	
	|_|	Conduct Part 135 airplane operations without a deicing/anti-icing procedure.
	
	
	A042

	
	
	|_|	Determine ground icing conditions for the purpose of flight [using an approved deicing/anti-icing procedure IAW CFR Section 135.227(b)(3)].
	
	
	A023

	
	SPECIAL OPERA-TIONS
	|_|	Conduct airplane air ambulance operations Part 135.
	
	
	A024

	
	
	|_|	Conduct Land and Hold Short Operations (LAHSO) at designated airports and specified runway configurations as identified by Air Traffic Services in Notice 7110.118, Appendix 1.
	
	
	A027

	
	
	|_|	Conduct Single Engine IFR (SEIFR) Passenger-Carrying Operations Under CFR Part 135.
	
	
	A046

	
	
	|_|	Conduct special en route IFR operations in Class G airspace.
	
	
	A014




Page 2–7 
Note: The term “FAR” in this document means “14 CFR Part”	https://avssharepoint.faa.gov/afs/aal/aalanc/shared documents/conformity worksheet[2]07312009dwd.doc
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	2.2
AIRCRAFT OPERATIONS
continued
	INSTRUCTIONS 
1.  If you want an operation described below, check the box to the left of its description.
	Document Requirements
	Procedures

	
	
	
	
	Training/
Skill

	
	
	
	2.  Then, look to see if a   appears to the right of the operation under “Procedures” and/or “Training/Skill” and revise your operating procedures and training manual and prepare to show proficiency as indicated.   The FSDO will provide any guidance you request.  
	
	
	OPSS
Ref
Par

	
	[bookmark: _Toc533324472][bookmark: _Toc533324653]PART B ENROUTE

	
	
	|_|	IFR en route operations.
	
	
	B032

	
	Class I Navi-gation
	[bookmark: _Hlt533219658]|_|	Using an area navigation system certified under one or more of the following Advisory Circulars:  AC 90-45A, 20-101C, 20-121A, 20-130A, 20-138.
	Complete Section 3.2.1 
AREA or Long Range NAV Systems: For these Operations Specifications
	
	
	B034

	
	
	|_|	In the U.S. Class A airspace using an area or long-range navigation system.
	
	
	
	B035

	
	Class II Navi-
gation
	|_|	Conduct using (dual) long-range navigation systems.
	
	
	
	B036

	
	
	|_|	Conduct operations in Central East Pacific (CEP) airspace.
	
	
	
	B037

	
	
	|_|	Conduct operations in North Pacific (NOPAC) airspace.
	
	
	
	B038

	
	
	|_|	Conduct operations in North Atlantic minimum navigation performance specifications (NAT/MNPS) airspace.
	
	
	
	B039

	
	
	|_|	Conduct operations in areas of magnetic unreliability.
	
	
	
	B040

	
	
	|_|	Conduct using single long-range navigation system (S-LRNS).
	
	
	
	B054

	
	
	|_|	Conduct extended overwater operations using a single long-range communication system (S-LRCS).
Complete Section 3.2.2 
Long-Range Communications System(s) (LRCS) For these Operations Specifications
	
	
	B045

	
	RVSM
	|_|	Conduct operations in reduced vertical separation minimum (RVSM) airspace.
	
	
	B046



	[bookmark: _Toc533324473][bookmark: _Toc533324654][bookmark: _Toc16496428]
AREAS OF OPERATION
	Operations Outside the Contiguous United States.  
(If yes, please list each country and oceanic area of operation)
	[bookmark: Check43]Yes |_|
	[bookmark: Check44]No |_|
	B050

	
	Enter “No change to B50” if appropriate

	
	     




	[bookmark: _Toc533324474][bookmark: _Toc533324655][bookmark: _Toc16496429]
PART C 
TERMINAL AREA OPERATIONS
	INSTRUCTIONS 
1.  If you want an operation described below, check the box to the left of its description.
	Document Requirements
	Procedures

	
	
	
	
	Training/
Skill

	
	
	
	2.  Then, look to see if a   appears to the right of the operation under “Procedures” and/or “Training/Skill” and revise your operating procedures and training manual and prepare to show proficiency as indicated.   The FSDO will provide any guidance you request.  
	
	
	OPSS
RefPar

	
	
	|_|	Conduct terminal instrument operations using specific procedures and landing minima for airplanes.
	
	
	C051

	
	
	|_|	Conduct Basic Instrument Approach procedure authorizations – all airports
	
	
	C052

	
	
	|_|	Conduct straight-in Category I approach procedures other than ILS, MLS, or GPS with specific IFR landing minimums for airplanes at all airports.
	
	
	C053

	
	
	|_|	Conduct IFR approach procedures using special IFR landing minimums for airplanes.
	
	
	C054

	
	
	|_|	Use IFR Takeoff Minimums, FAR 135 Airplane Operations - All Airports.
	
	
	C057

	
	
	|_|	Conduct foreign terminal instrument procedures with special restrictions for airplanes.
	
	
	C058

	
	RNAV
	|_|	Conduct airplane operations using published RNAV (VOR/DME) instrument approach procedures with an area navigation system.  Complete Section 3.2.1 
AREA or Long Range NAV Systems: For these Operations Specifications
	
	
	C063

	
	
	|_|	Conduct nonscheduled passenger and/or all-cargo, special terminal area IFR airplane operations in Class G airspace and at airports without an operating control tower.
	
	
	C064

	
	
	|_|	Use powerplant reversing systems for rearward taxi in specific airplane operations.
	
	
	C065

	
	
	|_|	Conduct turbojet airplane operations with tailwind components in excess of 10 knots but not to exceed 15 knots.
	
	
	C066

	
	
	|_|	Conduct turbojet airplane takeoff operations with tailwind components of 10 knots or less.
	
	
	C069

	
	
	|_|	Engage the autopilot after takeoff and initial climb at an altitude lower than specified for en route operations by Title 14 CFR Section 135.93 (a).
	
	
	C071

	
	
	|_|	Conduct engine-out departure procedures with approved 10-minute takeoff thrust time limits.
	
	
	C072

	
	VNAV
	|_|	Conduct IFR airplane approach procedures using vertical navigation (VNAV) utilizing a published MDA as a DA(H).  Complete Section 3.2.1 
AREA or Long Range NAV Systems: For these Operations Specifications
	
	
	C073

	
	
	|_|	Conduct airplane Category I, ILS, MLS, or GLS approach procedures with specific IFR landing minimums.
	
	
	C074

	
	
	|_|	Conduct airplane circle-to-land approach maneuvers using IFR Category I landing minimums.
	
	
	C075

	
	
	|_|	Conduct airplane contact approaches using IFR Category I landing minimums.
	
	
	C076

	
	
	|_|	Conduct certain Part 135 turbojet operations in the terminal area using visual flight rules.
	
	
	C077

	
	
	|_|	Conduct takeoffs in weather minimums below Category I takeoff minimums for FAR 135 airplane operations.
	
	
	C079




	[bookmark: _Toc533324475][bookmark: _Toc533324656][bookmark: _Toc16496430]
PART D  MAINTENANCE PROGRAM
	INSTRUCTIONS 
1.  If you want an operation described below, check the box to the left of its description.
	Document Requirements
	Procedures

	
	
	
	
	Training/
Skill

	
	

	
	2.  Then, look to see if a   appears to the right of the operation under “Procedures” and/or “Training/Skill” and revise your operating procedures and training manual and prepare to show proficiency as indicated.   The FSDO will provide any guidance you request.  
	
	
	OPSS
Ref
Par

	
	CAMP
135.411(a)(2) 
and 135.423
	|_|	Conduct continuous airworthiness maintenance programs.  (CAMP) (required for 10-or-more operators, optional for all others).  
	
	
	D072

	
	
	|_|	Use the provisions of contractual agreements limited to specific maintenance functions.
	
	
	D078

	
	
	|_|	Conduct ferry flights under special flight permits with continuing authorization.
	
	
	D084

	
	
	|_|	Use maintenance time limitations for operators without a reliability program.
	
	
	D089

	
	AAIP
134.419
	|_|	Use an approved aircraft inspection program (AAIP).  (required for Turbine powered multi-engine aircraft, optional for others) 
	
	
	D073

	
	RVSM
	|_|	Use an approved maintenance program for listed airplanes used in operations in designated RVSM airspace.
	
	
	D092

	
	MEL
135.179
	|_|	Use an approved minimum equipment list (MEL).  Inoperable instruments and equipment: 
	
	
	D095

	
	NINE OR LESS PAX SEATS 
135.411(a)(1).
	|_| Annual & 100 Hour Inspections
FAR Parts 91.409(a) & (b)
	|_|	Additional maintenance requirements of 14 CFR Section 135.421 applicable for aircraft engine, propeller, and propeller control (governor).
	
	
	D101

	
	
	|_| Progressive Inspections 
FAR Part 91.409(d)
	|_|	Additional maintenance requirements of 14 CFR Section 135.421 applicable for single engine IFR.
	
	
	D103

	
	
	|_| Manufacturers Program
FAR 91.409 (f3)
	|_|	Additional maintenance requirements of 14 CFR Section 135.421 applicable for emergency equipment.
	
	
	D104






	[bookmark: _Toc533324476][bookmark: _Toc533324657][bookmark: _Toc16496431]
SPECIAL OPERATIONS SPECIFICA
TIONS FOR HELICOPTERS
	INSTRUCTIONS 
1.  If you want an operation described below, check the box to the left of its description.
	Document Requirements
	Procedures

	
	
	
	
	Training/
Skill

	
	
	2.  Then, look to see if a   appears to the right of the operation under “Procedures” and/or “Training/Skill” and revise your operating procedures and training manual and prepare to show proficiency as indicated.   The FSDO will provide any guidance you request.  
	
	
	OPSS
Ref
Par

	
	|_|	Use An Approved Security Program In Helicopter Operations.  (to Deplane PAX in sterile areas) 
	
	
	A017

	
	|_|	Conduct helicopter air ambulance operations in accordance with CFR 14 Part 135.
	
	
	A021

	
	|_|	Conduct helicopter night vision goggle operations.
	
	
	A050

	
	|_|	Use an approved maintenance program for its helicopter night vision goggle operations.
	
	
	D093

	
	|_|	Use aircraft with nine or less passenger seats with the additional maintenance requirements of 14 CFR Section 135.421 applicable for rotorcraft operations.
	
	
	D102

	
	|_|	Conduct terminal flight operations under instrument flight rules - helicopter.
	
	
	H101

	
	|_|	Conduct operations using basic instrument approach procedures for helicopters.
	
	
	H102

	
	|_|	Conduct Category I IFR landings other than airborne radar approaches - helicopter.
	
	
	H103

	
	|_|	Conduct IFR helicopter en route descent (HEDA) procedures.
	
	
	H104

	
	|_|	Use alternate airport IFR weather minimums - helicopter.
	
	
	H105

	
	|_|	Conduct helicopter operations using standard takeoff minimums under Part 135.
	
	
	H106

	
	|_|	Use special restrictions for foreign terminal instrument procedures - helicopter.
	
	
	H107

	
	|_|	Conduct helicopter Category II operations.
	
	
	H108

	
	|_|	Conduct helicopter Category III operations.
	
	
	H109

	
	|_|	Use flight control guidance systems for aircraft automatic landing operations - helicopter.
	
	
	H110

	
	|_|	Use manually flown flight control guidance systems certified for aircraft landing operations - helicopter.
	
	
	H111

	
	|_|	Conduct helicopter approach operations using an area navigation system.
	
	
	H112

	
	|_|	Conduct nonscheduled passenger and all-cargo (scheduled and nonscheduled) special terminal area IFR rotorcraft operations in Class G airspace.
	
	
	H113

	
	|_|	Use special airport authorizations, limitations, and provisions - helicopter.
	
	
	H114

	
	|_|	Conduct helicopter operations using lower than standard takeoff minimums under Part 135.
	
	
	H116

	
	|_|	Conduct helicopter Category I, ILS, MLS, or GLS approach procedures with specific IFR landing minimums.
	
	
	H117

	
	|_|	Conduct helicopter circle-to-land maneuvers using IFR Category I landing minimums.
	
	
	H118

	
	|_|	Conduct helicopter contact approaches using IFR Category I landing minimums.
	
	
	H119

	
	|_|	Conduct special non CFR Part 97 instrument approach or departure rotorcraft operations specified for the following airports.
	
	
	H122


SECTION 2	REQUEST FOR OPERATIONS SPECIFICATIONS 
FOR THIS AIRCRAFT (continued)


	NOTICE:  PART NUMBERS AND DOCUMENT NUMBERS MUST BE COMPLETE AND ACCURATE.  



	
	[bookmark: _Toc533324477][bookmark: _Toc533324658][bookmark: _Toc16496432]
ADDITIONAL REQUIRED AIRCRAFT INFORMATION 

For Operations under Part 135.411(a)(1) Only 
(“Nine-or-Less Operations”)
	AIRCRAFT : Enter the Aircraft maintenance publication (identification or part number) here:
	
	Aircraft Maintenance 
Manual & 
	[bookmark: Text7][bookmark: _Hlt14229607]     

	
	
	
	Revision Level
	     

	
	
	
	Date
	     

	
	ITEM
	Make & 
Model
	Maintenance/Overhaul Document ID or Part Number
(Read Note 1)
	Time In Service Document ID or Part Number
(Read Note 2)
	TIME-IN-SERVICE 
INTERVAL

	
	ENGINE 
(Left or Single Engine)
	[bookmark: Text8]     
	     
	     
	     

	
	ENGINE 
(Right if applicable)
	     
	     
	     
	     

	
	PROPELLER 
(Left or Single Engine)
	     
	     
	     
	     

	
	PROPELLER 
(Right if applicable)
	     
	     
	     
	     

	
	PROPELLER GOVERNOR 
(Left or Single Engine)
	     
	     
	     
	     

	
	PROPELLER GOVERNOR 
(Right if applicable)
	     
	     
	     
	     

	
	PRIMARY GOVERNOR 
	     
	     
	     
	     

	
	OVERSPEED GOVERNOR 
	     
	     
	     
	     


NOTE 1.  Please enter the exact name and identification or part number of the publication(s), including revision level, under which the item will be maintained (normally these are the airframe and the engine, propeller, and governor service manuals).  
NOTE 2.  Please identify the manufacturer's publication(s) by exact number and title that specify the overhaul /replacement time, or time-in-service interval for the item.  This is often a service bulletin.  
	1.2 [bookmark: _Toc533324478][bookmark: _Toc533324659][bookmark: _Toc16496433]
MAINTENANCE HISTORY 
	Before this application, the aircraft was maintained under the following maintenance/inspection program:  (Please check)

	
	FAR Parts 43, 91 and 91.409
	|_| (a) Annual inspections   |_| (b) 100 Hour Inspections 
|_| (d) Progressive inspections, or

	
	
	Air Carrier’s Program 
|_| (f1) or |_| (f2) 
	Manufacturers Program |_| (f3) or
	Other Approved Program 
|_| (f4)

	1.3 [bookmark: _Toc16496434]
PRIMARY MAINTENANCE BASE
	Location of the aircraft records and, 
If applicable,* the office of the Director Of Maintenance 
*Optional for Single Pilot and Single Pilot-in-Command Operators
	     





	1.4 [bookmark: _Toc16496435][bookmark: _Ref16496944]MAJOR ALTERATIONS
	A/C Make/Model       
Registration      N     



LIST ALL MAJOR ALTERATIONS THAT CURRENTLY APPLY TO THE AIRCRAFT; 
use additional copies of this page as needed.  
	DATE
337 block 7
	Instructions For Continued Airworthiness

	
	Apply 
(Yes or No)
	Field Approval

	
	
	in Block 3 
(Yes or No)
	Flight Manual Supplement

	
	
	
	Required (Yes or No)
	Brief Description of the Major Alteration

	     
	   
	   
	   
	     

	     
	   
	   
	   
	     

	     
	   
	   
	   
	     

	     
	   
	   
	   
	     

	     
	   
	   
	   
	     

	     
	   
	   
	   
	     

	     
	   
	   
	   
	     

	     
	   
	   
	   
	     

	     
	   
	   
	   
	     

	     
	   
	   
	   
	     

	     
	   
	   
	   
	     

	     
	   
	   
	   
	     





	1.5 [bookmark: _Toc16496436]PRESSURE CYLINDERS AND SPHERES



List all Pressure Cylinders and Spheres installed as Aircraft Equipment
Please refer to HBAW 02-01, July 16, 2002, (or later revision) for details.  
	Part Number
	Description or 
Part Name
	Manufacturer’s Maintenance Document
	Applicable limitations and provisions including current due dates.

	     
	     
	     
	     

	     
	     
	     
	     

	     
	     
	     
	     

	     
	     
	     
	     

	     
	     
	     
	     

	     
	     
	     
	     

	     
	     
	     
	     

	     
	     
	     
	     


SECTION 2	REQUEST FOR OPERATIONS SPECIFICATIONS 
FOR THIS AIRCRAFT (continued)

Page 2–6
Note: The term “FAR” in this document means “14 CFR Part”	https://avssharepoint.faa.gov/afs/aal/aalanc/shared documents/conformity worksheet[2]07312009dwd.doc
Formdate 
[bookmark: _Toc533324479][bookmark: _Toc533324660][bookmark: _Toc16496437]AIRCRAFT COMPLIANCE STATEMENT FOR 135 OPERATIONS
	[bookmark: _Toc533324480][bookmark: _Toc533324661][bookmark: _Toc534767950][bookmark: _Toc534768020][bookmark: _Toc534778177][bookmark: _Toc534778315][bookmark: _Toc534789448][bookmark: _Toc16496438]ALL AIRCRAFT
	A/C Make/Model       
Registration      N     


INSTRUCTIONS FOR SECTION 3:
· Please refer to FAR 135 Subpart C Aircraft and Equipment, and Far 91 as applicable, for the specific requirements of the items listed below
· Check the box next to the item to indicate that it meets the requirements of the rule.  
· Provide all additional information indicated.  
	[bookmark: _Toc534767951][bookmark: _Toc534768021][bookmark: _Toc534778316][bookmark: _Toc534789449]
General requirements
	135.143
	|_|	(a)  For each item initialed, the applicant certifies that the equipment meets the applicable Federal Aviation Regulations. Indicate items that do not apply by “NA.”

	
	
	|_|	(b)  All equipment not originally installed by the aircraft manufacturer meets FAA approved data shown by FAA Form(s) 337 which are listed in Section 2.10 of this form and are available for inspection by the FSDO.  

	
	
	

	[bookmark: _Toc533579327][bookmark: _Toc534767953][bookmark: _Toc534768023][bookmark: _Toc534778318][bookmark: _Toc534784888][bookmark: _Toc534786836][bookmark: _Toc534786919][bookmark: _Toc534789451][bookmark: _Toc2756206][bookmark: _Toc3695955][bookmark: _Toc6902495][bookmark: _Toc14228108]
ATC Transponders
	
	|_|	 (c)   ATC 
Transponder
	Make & Model
	Date Installed

	[bookmark: _Toc533579328][bookmark: _Toc534767954][bookmark: _Toc534768024][bookmark: _Toc534778319][bookmark: _Toc534784889][bookmark: _Toc534786837][bookmark: _Toc534786920][bookmark: _Toc534789452][bookmark: _Toc2756207][bookmark: _Toc3695956][bookmark: _Toc6902496][bookmark: _Toc14228109]
	
	#1
	     
	     

	[bookmark: _Toc533579329][bookmark: _Toc534767955][bookmark: _Toc534768025][bookmark: _Toc534778320][bookmark: _Toc534784890][bookmark: _Toc534786838][bookmark: _Toc534786921][bookmark: _Toc534789453][bookmark: _Toc2756208][bookmark: _Toc3695957][bookmark: _Toc6902497][bookmark: _Toc14228110]
	
	#2
	     
	      

	[bookmark: _Toc534767957][bookmark: _Toc534768027][bookmark: _Toc534778322][bookmark: _Toc534789455]
Equipment requirements: General
	135.144
	|_|	List all portable electronic devices intended to be used by the Flight Crew  


	
	135.147
	|_|   Dual controls are installed

	[bookmark: _Toc533579332][bookmark: _Toc534767958][bookmark: _Toc534768028][bookmark: _Toc534778323][bookmark: _Toc534784893][bookmark: _Toc534786841][bookmark: _Toc534786924][bookmark: _Toc534789456][bookmark: _Toc2756211][bookmark: _Toc3695960][bookmark: _Toc6902500][bookmark: _Toc14228113]
	135.149
	[bookmark: Check15][bookmark: Check16]|_|	(a)  Altimeter(s): Sensitive & adjustable for barometric pressure 
(b)    |_| Carburetor: Heat/Deice or     |_| Pressure Carburetor: Alternate air source 
|_|	(c)  For Turbojet airplanes: Third artificial horizon installed according to FAR 121.305(j)

	[bookmark: _Toc534767959][bookmark: _Toc534768029][bookmark: _Toc534778324][bookmark: _Toc534789457]
Performance requirements:
	135.181
	|_|	Aircraft operated over‑the‑top or in IFR conditions 

	[bookmark: _Toc533579334][bookmark: _Toc534767960][bookmark: _Toc534768030][bookmark: _Toc534778325][bookmark: _Toc534784895][bookmark: _Toc534786843][bookmark: _Toc534786926][bookmark: _Toc534789458][bookmark: _Toc2756213][bookmark: _Toc3695962][bookmark: _Toc6902502][bookmark: _Toc14228115]
	135.183
	|_|	Land aircraft operated over water.

	[bookmark: _Toc534767961][bookmark: _Toc534768031][bookmark: _Toc534778326][bookmark: _Toc534789459]
Empty weight and center of gravity:
	135.185
	Currency requirement 
[bookmark: Text9]	For multiengine aircraft:  Date Last Weighed:         .

	[bookmark: _Toc533324481][bookmark: _Toc533324662][bookmark: _Toc534767962][bookmark: _Toc534768032][bookmark: _Toc534778327][bookmark: _Toc534789460]
Emergency Equipment
	135.155
	FIRE EXTINGUISHERS

	1.6 [bookmark: _Toc533579337][bookmark: _Toc534767963][bookmark: _Toc534768033][bookmark: _Toc534768223][bookmark: _Toc534771516][bookmark: _Toc534778178][bookmark: _Toc534778328][bookmark: _Toc534784898][bookmark: _Toc534786846][bookmark: _Toc534786929][bookmark: _Toc534789461][bookmark: _Toc2756216][bookmark: _Toc3695965][bookmark: _Toc6902505][bookmark: _Toc14228118][bookmark: _Toc14229332][bookmark: _Toc16496080][bookmark: _Toc16496259][bookmark: _Toc16496439]
	
	
	Make/Model
	Maintenance Document
	Aircraft Location

	1.7 [bookmark: _Toc533579338][bookmark: _Toc534767964][bookmark: _Toc534768034][bookmark: _Toc534768224][bookmark: _Toc534771517][bookmark: _Toc534778179][bookmark: _Toc534778329][bookmark: _Toc534784899][bookmark: _Toc534786847][bookmark: _Toc534786930][bookmark: _Toc534789462][bookmark: _Toc2756217][bookmark: _Toc3695966][bookmark: _Toc6902506][bookmark: _Toc14228119][bookmark: _Toc14229333][bookmark: _Toc16496081][bookmark: _Toc16496260][bookmark: _Toc16496440]
	
	1
	[bookmark: Text10]     
	     
	     

	[bookmark: _Toc533579339][bookmark: _Toc534767965][bookmark: _Toc534768035][bookmark: _Toc534778330][bookmark: _Toc534784900][bookmark: _Toc534786848][bookmark: _Toc534786931][bookmark: _Toc534789463][bookmark: _Toc2756218][bookmark: _Toc3695967][bookmark: _Toc6902507][bookmark: _Toc14228120]
	
	2
	     
	     
	     

	[bookmark: _Toc533579340][bookmark: _Toc534767966][bookmark: _Toc534768036][bookmark: _Toc534778331][bookmark: _Toc534784901][bookmark: _Toc534786849][bookmark: _Toc534786932][bookmark: _Toc534789464][bookmark: _Toc2756219][bookmark: _Toc3695968][bookmark: _Toc6902508][bookmark: _Toc14228121]
	
	3
	     
	     
	     

	[bookmark: _Toc533579341][bookmark: _Toc534767967][bookmark: _Toc534768037][bookmark: _Toc534778332][bookmark: _Toc534784902][bookmark: _Toc534786850][bookmark: _Toc534786933][bookmark: _Toc534789465][bookmark: _Toc2756220][bookmark: _Toc3695969][bookmark: _Toc6902509][bookmark: _Toc14228122]
	91.205
(b)(12)
	APPROVED PERSONAL FLOATATION GEAR 
Note: This equipment is required for operations in coastal areas.  It need not meet 135.167

	[bookmark: _Toc533579342][bookmark: _Toc534767968][bookmark: _Toc534768038][bookmark: _Toc534778333][bookmark: _Toc534784903][bookmark: _Toc534786851][bookmark: _Toc534786934][bookmark: _Toc534789466][bookmark: _Toc2756221][bookmark: _Toc3695970][bookmark: _Toc6902510][bookmark: _Toc14228123]
	
	Make Model:
	             
	No Installed
	  
	[bookmark: Check60]|_| one for each seat.

	
	91.207
	Emergency Locator Transmitter

	
	
	Make/
Model
	     
	ELT 
Type
	     
	TSO 
Number
	     

	[bookmark: _Toc534767969][bookmark: _Toc534768039][bookmark: _Toc534778334][bookmark: _Toc534789467]
Oxygen Equipment 
	135.157
	[bookmark: Check61]|_| Meets all requirements

	[bookmark: _Toc534767970][bookmark: _Toc534768040][bookmark: _Toc534778335][bookmark: _Toc534789468]
Passenger carrying under VFR at night or VFR over‑the‑top conditions
	135.159
	|_|  (a)  Gyroscopic Rate-of-Turn indicator
|_|  (b)  Slip skid indicator
|_|  (c)  Gyroscopic bank-and-pitch indicator
|_|  (d)  Gyroscopic direction indicator
	|_|  (e)  Generators meeting FAR specifications
      (f)  For Night Flight Authorization 
|_|  Anti collision light system 
|_|  Instrument lights 
|_|  2 "D" Cell flashlight or equivalent 

	[bookmark: _Toc534767971][bookmark: _Toc534768041][bookmark: _Toc534778336][bookmark: _Toc534789469]
VFR Radio and navigational equipment 
	135.161
	
	Make/Model
	
	Make/Model

	[bookmark: _Toc3695974][bookmark: _Toc6902514][bookmark: _Toc14228127]
	
	VHF 
COM 1  
	     	|_| 8.33 Khz 
Spacing
	DME 1  
	     

	[bookmark: _Toc533579346][bookmark: _Toc534767972][bookmark: _Toc534768042][bookmark: _Toc534778337][bookmark: _Toc534784907][bookmark: _Toc534786855][bookmark: _Toc534786938][bookmark: _Toc534789470][bookmark: _Toc2756225][bookmark: _Toc3695975][bookmark: _Toc6902515][bookmark: _Toc14228128]
	
	VOR 1 
	     	|_| FM 
Imunity
	ADF 1 
	     





	[bookmark: _Toc533324482][bookmark: _Toc533324663]3.1  
ALL AIRCRAFT (continued)
	A/C Make/Model       
Registration      N     



	[bookmark: _Toc534767973][bookmark: _Toc534768043][bookmark: _Toc534778338][bookmark: _Toc534789471]
Passengers Under IFR
	135.163
	[bookmark: Check7]|_|  (a)  Vertical speed indicator
[bookmark: Check8]|_|  (b)  Free air temperature indicator
[bookmark: Check9]|_|  (c)  Heated pitot tube for each airspeed indicator
[bookmark: Check10]|_|  (d)  Gyroscopic power source indicator or power failure warning indicator
	[bookmark: Check11]|_| (e)  Alternate static source 
	See Order 8340.1a chg 81, app 14, par 34-31 for exceptions
[bookmark: Check12]|_| (f)  Single-Engine aircraft 
	(Generator/load combination as specified)
[bookmark: Check13]|_| (g)  Multi-engine aircraft: 
	(two generators loaded as specified)
[bookmark: Check14]|_| (h)  Two independent sources of energy as specified to power gyroscopic instruments

	[bookmark: _Toc534767974][bookmark: _Toc534768044][bookmark: _Toc534778339][bookmark: _Toc534789472]
Radio and Navigational Equipment: IFR Operations
	135.165
	Make/Model
	|_|   two microphones      
|_|   Marker Beacon Receiver
|_|   two headsets or     
|_|   one headset and one speaker

	[bookmark: _Toc534767975][bookmark: _Toc534768045][bookmark: _Toc534778340][bookmark: _Toc534784910][bookmark: _Toc534786858][bookmark: _Toc534786941][bookmark: _Toc534789473][bookmark: _Toc2756228][bookmark: _Toc3695978][bookmark: _Toc6902518][bookmark: _Toc14228131]
	
	VHF COM 2
	     	|_| 8.33 Khz 
Spacing
	

	[bookmark: _Toc534767976][bookmark: _Toc534768046][bookmark: _Toc534778341][bookmark: _Toc534784911][bookmark: _Toc534786859][bookmark: _Toc534786942][bookmark: _Toc534789474][bookmark: _Toc2756229][bookmark: _Toc3695979][bookmark: _Toc6902519][bookmark: _Toc14228132]
	
	VOR NAV 2
	     	|_| FM 
Imunity
	


[bookmark: _Toc533324483][bookmark: _Toc533324664][bookmark: _Toc534767977][bookmark: _Toc534768047][bookmark: _Toc534778180][bookmark: _Toc534778342][bookmark: _Toc534789475][bookmark: _Ref14227634][bookmark: _Toc16496441]RNAV AND EXTENDED OVERWATER OPERATIONS
	[bookmark: _Ref533226788][bookmark: _Toc533324484][bookmark: _Toc533324665][bookmark: _Toc534767978][bookmark: _Toc534768048][bookmark: _Hlt534783859][bookmark: _Toc534778343][bookmark: _Toc534789476][bookmark: _Ref14227792]
AREA or Long Range NAV Systems:
	135.165
	Radio and navigational equipment for Extended Overwater Operation Authorization

	[bookmark: _Toc534767979][bookmark: _Toc534768049][bookmark: _Toc534778344][bookmark: _Toc534784914][bookmark: _Toc534786945][bookmark: _Toc534789477][bookmark: _Toc2756232][bookmark: _Toc3695982][bookmark: _Toc6902522][bookmark: _Toc14228135]
	
	
	Make/Model
	SENSORS -- INDICATE ALL
	APPROVED FOR

	[bookmark: _Toc534767980][bookmark: _Toc534768050][bookmark: _Toc534778345][bookmark: _Toc534784915][bookmark: _Toc534786946][bookmark: _Toc534789478][bookmark: _Toc2756233][bookmark: _Toc3695983][bookmark: _Toc6902523][bookmark: _Toc14228136]
	
	1
	       /       .

Date 
Installed        .
	|_|  Flight Management System or 
|_|  NAV Management System
|_|  Loran C   |_|  GPS   |_|  INS/IRS 
|_|  OTHER      
|_|  SHORT-RANGE RNAV 
|_|  VOR/DME  or
|_|  DME/DME-FMS
	|_| Enroute/Terminal
|_| Non-Precision Approaches
|_| Remote/Oceanic 
|_| RNP TYPE(s)      
Time Limits      
|_| BRNAV  
|_| VNAV

	[bookmark: _Toc534767981][bookmark: _Toc534768051][bookmark: _Toc534778346][bookmark: _Toc534784916][bookmark: _Toc534786947][bookmark: _Toc534789479][bookmark: _Toc2756234][bookmark: _Toc3695984][bookmark: _Toc6902524][bookmark: _Toc14228137]
	
	2
	       /       .

Date 
Installed        .
	|_|  Flight Management System or 
|_|  NAV Management System
|_|  Loran C   |_|  GPS   |_|  INS/IRS 
|_|  OTHER      
|_|  SHORT-RANGE RNAV 
|_|  VOR/DME  or
|_|  DME/DME-FMS
	|_| Enroute/Terminal
|_| Non-Precision Approaches
|_| Remote/Oceanic 
|_| RNP TYPE(s)     
Time Limits      
|_| BRNAV  
|_| VNAV

	[bookmark: _Toc534767982][bookmark: _Toc534768052][bookmark: _Toc534778347][bookmark: _Toc534784917][bookmark: _Toc534786948][bookmark: _Toc534789480][bookmark: _Toc2756235][bookmark: _Toc3695985][bookmark: _Toc6902525][bookmark: _Toc14228138]
	
	3
	       /       .

Date 
Installed        .
	|_|  Flight Management System or 
|_|  NAV Management System
|_|  Loran C   |_|  GPS   |_|  INS/IRS 
|_|  OTHER      
|_|  SHORT-RANGE RNAV 
|_|  VOR/DME  or
|_|  DME/DME-FMS
	|_| Enroute/Terminal
|_| Non-Precision Approaches
|_| Remote/Oceanic 
|_| RNP TYPE(s)     
Time Limits      
|_| BRNAV  
|_| VNAV

	[bookmark: _Ref533228859][bookmark: _Toc533324485][bookmark: _Toc533324666][bookmark: _Hlt534781486][bookmark: _Toc534767983][bookmark: _Toc534768053][bookmark: _Toc534778348][bookmark: _Hlt534781598][bookmark: _Toc534789481][bookmark: _Ref14227811]
Long-Range Communications System(s) (LRCS)
	
	
	Make/Model
	LRCS Type
	Date Installed

	[bookmark: _Toc534767984][bookmark: _Toc534768054][bookmark: _Toc534778349][bookmark: _Toc534784919][bookmark: _Toc534786950][bookmark: _Toc534789482][bookmark: _Toc2756237][bookmark: _Toc3695987][bookmark: _Toc6902527][bookmark: _Toc14228140]
	
	1
	       /      .
	|_| HF   |_| SAT/COM   |_| DATALINK   |_| OTHER
	     

	[bookmark: _Toc534767985][bookmark: _Toc534768055][bookmark: _Toc534778350][bookmark: _Toc534784920][bookmark: _Toc534786951][bookmark: _Toc534789483][bookmark: _Toc2756238][bookmark: _Toc3695988][bookmark: _Toc6902528][bookmark: _Toc14228141]
	
	2
	       /      .
	|_| HF   |_| SAT/COM   |_| DATALINK   |_| OTHER
	     

	[bookmark: _Toc534767986][bookmark: _Toc534768056][bookmark: _Toc534778351][bookmark: _Toc534784921][bookmark: _Toc534786952][bookmark: _Toc534789484][bookmark: _Toc2756239][bookmark: _Toc3695989][bookmark: _Toc6902529][bookmark: _Toc14228142]
	
	3
	       /      .
	|_| HF   |_| SAT/COM   |_| DATALINK   |_| OTHER
	     

	[bookmark: _Hlt533226838][bookmark: _Toc534767987][bookmark: _Toc534768057][bookmark: _Toc534778352][bookmark: _Toc534789485]
Airworthiness and Operating Limitations
	
	For each item listed above in sections 3.2.1, and 3.2.2 provide the following:
|_|	Copies of the portions of the installation approval documents (original Equipment List or FAA Form 337) and
|_|	Flight Manual Supplements that show the make and model of the equipment and approval for the requested operation.  Contact the FSDO if there are any questions.

	[bookmark: _Toc533324486][bookmark: _Toc533324667][bookmark: _Toc534767988][bookmark: _Toc534768058][bookmark: _Toc534778353][bookmark: _Toc534789486]
Emergency equipment Extended overwater operations
	135.167
	|_|	(a)  The following are conspicuously marked and easily accessible to the occupants if ditching occurs:

	[bookmark: _Toc534767989][bookmark: _Toc534768059][bookmark: _Toc534778354][bookmark: _Toc534784924][bookmark: _Toc534786955][bookmark: _Toc534789487][bookmark: _Toc2756242][bookmark: _Toc3695992][bookmark: _Toc6902532][bookmark: _Toc14228145]
	
	
	Make/Model
	Maintenance Document ID

	[bookmark: _Toc534767990][bookmark: _Toc534768060][bookmark: _Toc534778355][bookmark: _Toc534784925][bookmark: _Toc534786956][bookmark: _Toc534789488][bookmark: _Toc2756243][bookmark: _Toc3695993][bookmark: _Toc6902533][bookmark: _Toc14228146]
	
	[bookmark: Check30]|_|	Life Preserver with Light for each occupant.
	      /      
	     

	[bookmark: _Toc534767991][bookmark: _Toc534768061][bookmark: _Toc534778356][bookmark: _Toc534784926][bookmark: _Toc534786957][bookmark: _Toc534789489][bookmark: _Toc2756244][bookmark: _Toc3695994][bookmark: _Toc6902534][bookmark: _Toc14228147]
	
	[bookmark: Check31]|_|	Life rafts as specified in 135.167(b) & (c).
	      /      
	     


[bookmark: _Ref533216498][bookmark: _Ref533216516][bookmark: _Hlt533216533]

	


PLEASE  COMPLETE  THIS  PAGE   ONLY  IF  APPLICABLE.



	[bookmark: _Toc533324487][bookmark: _Toc533324668][bookmark: _Toc534767992][bookmark: _Toc534768062][bookmark: _Toc534778181][bookmark: _Toc534778357][bookmark: _Toc534789490][bookmark: _Toc16496442]TURBINE-POWERED, TURBOJET, AND/OR TEN-OR-MORE PASSENGER AIRCRAFT.
 
	A/C Make/Model       
Registration      N     



	[bookmark: _Toc534778358][bookmark: _Toc534789491]
Proving Test Flights
	135.145
	|_|
	NOT REQUIRED
	|_|  REQUIRED
	|_|  Proving test plan is scheduled on page 1-1
|_|  Proving tests are scheduled on page 1-1
|_|  Request for deviation is scheduled on page 1-1

	[bookmark: _Toc534778359][bookmark: _Toc534789492]
Additional Equipment Requirements
	135.150
	|_|	Public address and crewmember interphone systems

	[bookmark: _Toc6902538][bookmark: _Toc14228151]
	
	
	Make/Model/Series
	Date Installed

	[bookmark: _Toc534778360][bookmark: _Toc534784930][bookmark: _Toc534786961][bookmark: _Toc534789493][bookmark: _Toc2756248][bookmark: _Toc3695998][bookmark: _Toc6902539][bookmark: _Toc14228152]
	135.151
	|_|
	Cockpit Voice Recorders
	     
	     

	[bookmark: _Toc534778361][bookmark: _Toc534784931][bookmark: _Toc534786962][bookmark: _Toc534789494][bookmark: _Toc2756249][bookmark: _Toc3695999][bookmark: _Toc6902540][bookmark: _Toc14228153]
	135.151(d)
	|_|
	Dual Headsets/Boom Mics
	     
	     

	[bookmark: _Toc534778362][bookmark: _Toc534784932][bookmark: _Toc534786963][bookmark: _Toc534789495][bookmark: _Toc2756250][bookmark: _Toc3696000][bookmark: _Toc6902541][bookmark: _Toc14228154]
	135.152
	|_|
	Flight Recorders
	     
	     

	[bookmark: _Toc534778363][bookmark: _Toc534784933][bookmark: _Toc534786964][bookmark: _Toc534789496][bookmark: _Toc2756251][bookmark: _Toc3696001][bookmark: _Toc6902542][bookmark: _Toc14228155]
	135.153
	|_|
	Ground Proximity Warning System
	     
	     

	[bookmark: _Toc534778364][bookmark: _Toc534784934][bookmark: _Toc534786965][bookmark: _Toc534789497][bookmark: _Toc2756252][bookmark: _Toc3696002][bookmark: _Toc6902543][bookmark: _Toc14228156]
	135.154
	|_|
	Terrain Awareness & Warning System (TAWS)
	     
	     

	[bookmark: _Toc534778365][bookmark: _Toc534784935][bookmark: _Toc534786966][bookmark: _Toc534789498][bookmark: _Toc2756253][bookmark: _Toc3696003][bookmark: _Toc6902544][bookmark: _Toc14228157]
	
	
	|_| Class A      |_| Class B
	
	

	[bookmark: _Toc3696004][bookmark: _Toc6902545][bookmark: _Toc14228158]
	135.158
	|_|
	Pitot heat indication systems

	[bookmark: _Toc534778366][bookmark: _Toc534789499]
Additional Airworthiness Requirements
	135.169
	(a)	For all large airplanes (more than 12,500 pounds, maximum certificated takeoff weight): The aircraft
|_|	is a commuter category airplane, or  
|_|	meets the additional requirements of FAR 121.213 through 121.283, and 121.307:  (SEE NOTE)
(b)	For Reciprocating-engine airplanes configured for ten-or-more passengers or 
For Turbopropeller-powered Small Airplanes configured for ten-or-more passengers:  
|_|	meets all applicable conditions specified in 135.169(b) (SEE NOTE)
NOTE:  Applicants must attach a conformity statement showing compliance with all additional rules indicated in the applicable paragraph above.
(c)	For all ten-or-more small airplanes  
state the maximum Passenger seating configuration  	     	
(d)	Cargo or baggage compartments:  All transport category airplanes type certificated after January 1, 1958. 
|_| each class C or D cargo compartments is not greater than 200 cubic ft in volume, or
|_| meets all applicable conditions specified in this 135.169(d)

	[bookmark: _Toc534778370][bookmark: _Toc534784940][bookmark: _Toc534786971][bookmark: _Toc534789503][bookmark: _Toc2756258][bookmark: _Toc3696009][bookmark: _Toc6902547][bookmark: _Toc14228160]
	135.170
	[bookmark: Check52]|_|	Materials for compartment interiors  

	[bookmark: _Toc534778371][bookmark: _Toc534784941][bookmark: _Toc534786972][bookmark: _Toc534789504][bookmark: _Toc2756259][bookmark: _Toc3696010][bookmark: _Toc6902548][bookmark: _Toc14228161]
	135.171
	[bookmark: Check53]|_|	Shoulder harness installation at flight crewmember stations 

	[bookmark: _Toc534778372][bookmark: _Toc534784942][bookmark: _Toc534786973][bookmark: _Toc534789505][bookmark: _Toc2756260][bookmark: _Toc3696011][bookmark: _Toc6902549][bookmark: _Toc14228162]
	135.173
	
	
	Make/Model/ Series 
	Date Installed

	[bookmark: _Toc534778373][bookmark: _Toc534784943][bookmark: _Toc534786974][bookmark: _Toc534789506][bookmark: _Toc2756261][bookmark: _Toc3696012][bookmark: _Toc6902550][bookmark: _Toc14228163]
	
	|_|
	Airborne thunderstorm detection equipment requirements
	     
	     

	[bookmark: _Toc534778374][bookmark: _Toc534784944][bookmark: _Toc534786975][bookmark: _Toc534789507][bookmark: _Toc2756262][bookmark: _Toc3696013][bookmark: _Toc6902551][bookmark: _Toc14228164]
	135.175.
	|_|
	Airborne weather radar equipment requirements
	     
	     

	[bookmark: _Toc534778375][bookmark: _Toc534784945][bookmark: _Toc534786976][bookmark: _Toc534789508][bookmark: _Toc2756263][bookmark: _Toc3696014][bookmark: _Toc6902552][bookmark: _Toc14228165]
	135.177
	[bookmark: Check54]|_|
	Emergency equipment requirements for aircraft having 
a passenger seating configuration of more than 19 passengers 

	[bookmark: _Toc534778376][bookmark: _Toc534784946][bookmark: _Toc534786977][bookmark: _Toc534789509][bookmark: _Toc2756264][bookmark: _Toc3696015][bookmark: _Toc6902553][bookmark: _Toc14228166]
	135.180
	|_|
	Traffic Alert and Collision Avoidance System
	     
	     

	[bookmark: _Toc534778377][bookmark: _Toc534784947][bookmark: _Toc534786978][bookmark: _Toc534789510][bookmark: _Toc2756265][bookmark: _Toc3696016][bookmark: _Toc6902554][bookmark: _Toc14228167]
	
	
	
	[bookmark: Check39][bookmark: Check40][bookmark: Check41][bookmark: Check42]|_| TCAS I    |_| TCAS II     
TCAS II Software Version 7 or higher?    |_| Yes   |_| No
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[bookmark: _Hlt533217462][bookmark: _Toc533324489][bookmark: _Toc533324670][bookmark: _Toc16496443]FAR 135 AIRWORTHINESS CHECKLIST
	We suggest you use this checklist frequently and especially before presenting the aircraft to the FAA for inspection or before an FAA check ride.

	[bookmark: Text18][bookmark: Text19]A/C Make and Model           	 Registration  N      


CHECK THE BOX TO INDICATE COMPLIANCE


	INSPECTION ITEM
	Check if the item meets all applicable FAR Requirements

	CERTIFICATES AND REGISTRATION

	|_|	The Registration Certificate is on board and current.

	|_|	The Airworthiness Certificate is on board and current.

	|_|	The Radio Station License is on board and current. 

	OPERATING LIMITATIONS

	|_|	FAA Approved Aircraft Flight Manual (AFM) or Pilots Operating Handbook is current, complete, and in serviceable condition.  

	|_|	AFM contains Flight Manual Supplements that are current and applicable to the installed Autopilot/Flight Director, Navigation equipment, and other installed equipment to which a Flight Manual supplement applies.

	|_|	All flight deck placards required by the Type Certificate or the AFM are secure and readable.  

	|_|	The flight deck contains all operating manuals and/or placards required by TC, STC, or FAA Form 337s.  

	|_|	All switches, circuit breakers, controls, etc., are properly labeled

	|_|	AFM contains current weight and balance data, and all obsolete weight and balance data is superseded; or, for aircraft not requiring an AFM, the current weight and balance and equipment list is in the aircraft.

	|_|	AFM contains a current and complete equipment list.

	|_|	For multiengine aircraft, the AFM contains a weighing record showing the aircraft was weighed within the last three years.  The record includes an equipment list, which describes the approved aircraft configuration at the time of weighing.  The weighing record has the signature and certificate number of the person or agency doing the work and the date of completion.  

	

	AIR CARRIER OPERATIONS DOCUMENTS

	|_|	Aircraft Maintenance Log (14 CFR 135.65) contains no open Mechanical Irregularities

	|_|	Minimum Equipment List is on board and current.

	|_|	Air Carrier Operations Manual is on board and Current.

	|_|	Deferred Maintenance Log contains no items deferred beyond the time allowed in the MEL.

	[bookmark: Text25]|_|	     

	PASSENGER SAFETY

	|_|	All internal cabin placards required by the Type Certificate or the AFM are secure and readable.  

	|_|	Passenger Briefing Cards meet 14 CFR 135 Requirements.

	|_|	Required emergency equipment is on board, properly stowed, and inspected.  

	[bookmark: Text21]|_|	     

	[bookmark: Text22]|_|	     

	[bookmark: Text23]|_|	     

	GENERAL AIRWORTHINESS

	|_|	The aircraft has the proper equipment and approval documentation required by 14 CFR 135 Sub-Part C.  All equipment is operating properly.

	|_|	All external placards, required by the Type Certificate or the AFM, are secure and readable.

	|_|	All cowl fasteners, screws, etc., are secure.

	|_|	Antennas are free from erosion.

	|_|	ADF Sense antenna is under spring tension.

	|_|	All static wicks installed, none broken except as allowed under MEL.  No bonding straps broken

	|_|	The aircraft Make, Model and Serial Number data are on the outside of the fuselage.

	|_|	All instruments, systems and equipment are operating properly; the aircraft is airworthy and legal to fly.

	|_|	Aircraft complies with it’s type certification basis (TC) to include comformity to any STC or alteration and is in condition for safe operation.

	MAINTENANCE RECORDS

	|_|	The maintenance records show that all airworthiness inspections are current including, Annual/100 hr or Programmed Inspection, Altimeter, Encoder, Static System, ATC Transponder, etc.

	|_|	All required maintenance, including maintenance of life limited items, is current.

	|_|	The maintenance records include an Airworthiness Directive (AD) Listing showing that all ADs are complied with including Recurring ADs.  The listing must comply with FAR 91.417(a)(i)(v)

	|_|	The maintenance records include entry for completion of this conformity inspection “This aircraft and its equipment conforms to the requirements of 14 CFR Part 135.25, including registration, current airworthiness certification, identification, and current airworthy condition for operation on Part 135 Certificate #______________.”  Entry must include date, aircraft total time, signature, certificate type and number. 




	I certify that, to the best of my knowledge, the information contained in this report is complete and accurate.  

	
	[bookmark: Text20]     

	Director of Maintenance
	Date
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