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Fueling Facility Monthly Audit
Fueling facilities that are frequented by MHI aircraft shall have a monthly audit using this checklist.  Results of the audit shall be kept on file for one year.  They audit may be performed by either a qualified pilot or mechanic.
Ref: ATA 103
[bookmark: _GoBack]Name of Facility: ______________________________________________      ICAO Code: ____________   

1. Ensure fuel truck has been inspected for contamination and recorded…………………………………….
2. Check condition of bonding cables, no frying, breaks and/or excessive corrosion…………………… 
3. Ensure Fueling nozzle has a bonding cable to attach to aircraft………………………………………………..
4. Ensure fueling point has been checked that day for contamination and results recorded….…….
5. Ensure fueling location has a proper fire extinguisher readily available………………………….………..
6. Are there any visible fuel leaks to include hoses and nozzles…………………………………………….……..
7. Check for appropriate decals such as No Smoking are present and legible………………………….…… 
8. Check any filters to ensure replacement is not overdue.  A Filter Due Replacement sticker should be readily visible…………………………………………………………………………………………………….………….………  

If suspected fuel contamination, contact the Director of Operations or Director of Maintenance for guidance and further testing.

Notes: _________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________________

Printed  Name________________________  Date __________________
Signature ___________________________________________________
image1.png
r«‘.: Maritime Helicopters




