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Pilot Training Certification

Bell Helicopter ASB 407-13-99
Rolls Royce CEB-A-72-6075

Subject: 20 Hour Engine Chip Plug Removal/Inspection/Installation 

This curriculum trains Bell 407 Pilots in the removal, inspection and re-installation of the two quick disconnect engine chip detectors on the Bell 407 Rolls Royce 250-C47B Engine. Training includes the recognition of metal accum- ulations on the chip detectors and proper reporting procedures for assessment, per instructions and procedures outlined in Rolls Royce CEB-A-72-6075.

Tools Required -  NONE

This Certifies that ___________________________________ has received instruction in order to remove, inspect, and re-install the two engine quick-disconnect chip detectors located on the engine gearbox. If there is evidence of metal on either or both chip detectors, it must be reported to the Maritime Helicopters Director of Maintenance and Director of Operations before further flight. Contact Rolls Royce Customer Support as outlined in CEB-A-72-6075. 


Pilots Name ________________________________________________
Certificate Number/Type _____________________________________
Date_____________


Instructing Mechanics Name __________________________________
Certificate Number/Type _____________________________________
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